

Reproducer to Recording Media Compatibility
	Reproducer/Sound box Type
	Needle/Stylus
	Record Type

	Any sound box with a mica diaphragm: Victor Exhibition; No. 2, No. 3, No. 4; Columbia No.5, No. 6, etc.
[image: ][image: ]
Exhibition and No.2 photos by Peter Poggi
[image: C:\Users\George\Desktop\APS006.jpg]
From The Columbia Phonograph Companion, Vol. II, by Robert Baumbach.
	Steel
Low tone
Medium tone
Loud tone
Spearpoint
Bamboo
Fiber
Tungs-tone
	Earlier than 1925
Acoustically recorded shellac, mostly laterally cut. Records manufactured before the introduction of electrical recording in 1925 are intended for mica diaphragm reproducers. Stick to acoustically recorded records from before 1925. The mica diaphragm is built to handle the low volume and frequency range of the acoustic discs. Playing post-1925 electrically recorded discs may delaminate the diaphragm and cause excessive movement of the needle in the groove, damaging the groove walls.




	Reproducer/Sound box Type
	Needle/Stylus
	Record Type

	Victor Orthophonic, Columbia Viva-Tonal (see above), any sound box with an aluminum diaphragm, etc.
[image: ]

	Steel, 
Spearpoint, 
Bamboo, 
Tungs-tone
	Any laterally cut, electrically recorded 78 made before 1937. You can play an acoustical recording with an orthophonic, but there is no real sound advantage. 

	
	Steel, 
Spearpoint,
 Bamboo, 
Tungs-tone
	Electric recordings made between 1925-1937 using the Western Electric Westrex recording system (Victor Orthophonic & Columbia Viva-Tonal specifically) are part of a balanced system.

	
	Steel Soft Tone, 
Bamboo
	Records made after 1937 were designed with a different recording curve made to generate a tiny piezo-electric spark in a Rochelle salt-crystal pickup. There is too much sound energy in that groove for an Orthophonic-style reproducer to handle efficiently. Records after 1937 can be played using a soft tone -tone needle but it’s not compatible with the Westrex system.



	Reproducer/Sound box Type
	Needle/Stylus
	Record Type

	Pathé
	Sapphire Ball
	Pathé uses a vertical cut groove that is U-shaped in cross-section and is tracked with a sapphire ball stylus.

	Edison Diamond Stylus
	Diamond
	Edison DD Vertical Cut. Edison ¼” discs use a groove that is V-shaped in cross-section and is tracked with a conical diamond stylus.



Differentiating between Acoustically and Electrically recorded records.
Assume you are looking at a disc and you do not recognize the artist nor know the production year. You can tell its shellac and not vinyl from the weight and thickness. BUT is there any physical or visual characteristic that can indicate whether it's acoustic or electrically recorded? 
You may be able to date the disc by examining the labels.  This is a great reference for this purpose.  http://majesticrecord.com/labelsvictor.htm
Often there is some reference to ‘Electrically Recorded’ or lightning bolts, etc. incorporated in the design. Some Victor records have “VE” (“Victor Electric”) printed on the label or engraved in the “run-out” area. Some of the last Victor “Batwing” labels have the word “Orthophonic” to the left of the spindle hole as they switched over to electric recording in 1925. The Victor “Scroll” label appeared on electrically recorded records from 1926 through 1937. 
A good rule of thumb regarding acoustic machines with mica diaphragms:
Avoid playing 78s with a lead in groove on the perimeter, which date from approx. 1934 and later. 78s with a lead in groove have a wider dynamic range and increased volume that a mica diaphragm just wasn’t designed to handle, even with soft tone needles.

If you must play later 78s on a mica diaphragm type of sound box, go easy on the later records and use the thorn or fiber needles.



Information provided by Gertie Maeder and George Paul, compiled by Peter Poggi. Please refer suggestions to peter.poggi@yahoo.com 
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S Gold Plated Brass Orthophonic Reproducer .
Photo by Peter Poggl e
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Columbia Concert Grand

Reproducer showing both

playing and needle loading
position

The Columbia Number 5 reproducer (left) and the larger
Columbia Number 6 Reproducer (right)

The New Columbia
Phonograph Reproducer
introduced in 1924

The Viva-Tonal Columbia
Phonograph Reproducer with
aluminum diaphragm
introduced 1926






Reproducer to 


Recording 


Media 


C


ompatibility


 


Information 


provided by Gertie Maeder


 


and George Paul, compiled 


by


 


Peter Poggi. Please


 


refer suggestions to 


peter.poggi@yahoo.com


 


 


Reproducer


/Sound box


 


Typ


e


 


N


eedle


/Stylus


 


Record Type


 


Any sound box


 


with a mica diaphragm: 


V


ictor


 


Exhibition


; 


No. 2


,


 


No. 3


,


 


No. 4


; 


Columbia No.5, 


No. 


6


, etc.


 


 


Exhibition and No.2 photos by 


Peter


 


Pog


g


i


 


 


From The Columbia Phonograph Companion


, Vol. II, by 


Robert Baumbach.


 


Steel


 


Low tone


 


Medium ton


e


 


Loud


 


tone


 


Spearpoint


 


Bamboo


 


Fiber


 


Tungs


-


tone


 


Earlier than 1925


 


Acoustically recorded s


hellac, 


mostly 


laterally cut


. 


Records


 


manufactured 


before the introduction of


 


electrical 


recording in 1925 are


 


i


ntended for 


mi


ca diaphragm reproducers.


 


S


tick to 


acousti


cally recorded records from 


before 1925. The mica diaphragm is 


built to handle the low volume and 


frequency range of the acoustic discs. 


Playing post


-


1925 


electrically 


recorded discs may 


delamin


ate th


e 


diaphragm


 


a


n


d cause excessive 


movement of the needle i


n the 


groove, damaging


 


the groove walls.


 


 


 




Reproducer to  Recording  Media  C ompatibility   Information  provided by Gertie Maeder   and George Paul, compiled  by   Peter Poggi. Please   refer suggestions to  peter.poggi@yahoo.com    

Reproducer /Sound box   Typ e  N eedle /Stylus  Record Type  

Any sound box   with a mica diaphragm:  V ictor   Exhibition ;  No. 2 ,   No. 3 ,   No. 4 ;  Columbia No.5,  No.  6 , etc.     Exhibition and No.2 photos by  Peter   Pog g i     From The Columbia Phonograph Companion , Vol. II, by  Robert Baumbach.  Steel   Low tone   Medium ton e   Loud   tone   Spearpoint   Bamboo   Fiber   Tungs - tone  Earlier than 1925   Acoustically recorded s hellac,  mostly  laterally cut .  Records   manufactured  before the introduction of   electrical  recording in 1925 are   i ntended for  mi ca diaphragm reproducers.   S tick to  acousti cally recorded records from  before 1925. The mica diaphragm is  built to handle the low volume and  frequency range of the acoustic discs.  Playing post - 1925  electrically  recorded discs may  delamin ate th e  diaphragm   a n d cause excessive  movement of the needle i n the  groove, damaging   the groove walls.  

   

